**MHT -CET-** **2021-2022** परीक्षा केंद्राकरीता मा आयुक्त महाराष्ट्र राज्य सामाईक प्रवेश परीक्षा कक्ष यांचे कडून ऑनलाईन अर्ज मागविण्यात आलेले होते. परीक्षा केंद्राकरीता आवश्यक असणा-या सोयीसुविधा खालील प्रमाणे आहेत.

**1. Hardware Requirement**

|  |  |  |
| --- | --- | --- |
| Candidate Machine Configuration --  | RAM - 4 GB recommended, 2 GB minimum  | Screen Resolution Support - 1024 X 768 or above  |
| Operating System - Windows 7 and above  | Browser - Internet Explorer 11.0  | Browser Settings - Internet Explorer (IE) Java Script enabled Pop-up blocker disabled  |
| Paste operations via script enabled Proxy disabled  | Other software - Net 3.5 and above Framework  | Adobe Reader  |
| Other Requirements - USB ports for storage devices to be disabled  | Wifi drivers to be disabled  | Full Admin rights to be given  |

**2. Monitor requirement** - NO CRT Monitor only TFT monitor min requirement is 15.6 inch

**3. Operating System:-**

|  |  |  |
| --- | --- | --- |
| Windows 7 (32bit/64bit) /Ubuntu 14.04 (32 bit)  | Browser:- Internet Explorer (IE) 9.0 or above (in windows )and Mozilla Firefox 50 (Linux)  | Other Required Softwares:- Adobe Reader and Flash player.  |
| net Framework 3.5 and above  | Full admin Rights required for the User.  | No other software should be installed in OS.  |
| Internet Connectivity should be isolated from the exam conducting LAB.  | Proxy Should be disable.  | Proxy Should be disable.  |
| Firewall should be enable.  | PC should be updated from ransomware patch.  |  |

 4.**Technical requirements**

|  |  |  |
| --- | --- | --- |
| CPU Hardware ( if available as above mention yes if not then give details of available configuration) | Monitor requirement ( if available as above mention yes if not then give details of available configuration) | CPU Operating System ( if available as above mention yes if not then give details of available configuration) |
| Primary netboot OS.Ileon OS (To be provided by TCS) for candidate machines | Backup linux Ubuntu 14.0.4 LTS | Internet connectivity to server |
| Network Configuration - STAR Topology / Network Cable – ACT 5E/CAT 6 /Connectors – RJ45v/Switches – Min 100 Mbps |