**MHT -CET-** **2021-2022** परीक्षा केंद्राकरीता मा आयुक्त महाराष्ट्र राज्य सामाईक प्रवेश परीक्षा कक्ष यांचे कडून ऑनलाईन अर्ज मागविण्यात आलेले होते. परीक्षा केंद्राकरीता आवश्यक असणा-या सोयीसुविधा खालील प्रमाणे आहेत.

**1. Hardware Requirement**

|  |  |  |
| --- | --- | --- |
| Candidate Machine Configuration -- | RAM - 4 GB recommended, 2 GB minimum | Screen Resolution Support - 1024 X 768 or above |
| Operating System - Windows 7 and above | Browser - Internet Explorer 11.0 | Browser Settings - Internet Explorer (IE) Java Script enabled Pop-up blocker disabled |
| Paste operations via script enabled Proxy disabled | Other software - Net 3.5 and above Framework | Adobe Reader |
| Other Requirements - USB ports for storage devices to be disabled | Wifi drivers to be disabled | Full Admin rights to be given |

**2. Monitor requirement** - NO CRT Monitor only TFT monitor min requirement is 15.6 inch

**3. Operating System:-**

|  |  |  |
| --- | --- | --- |
| Windows 7 (32bit/64bit) /Ubuntu 14.04 (32 bit) | Browser:- Internet Explorer (IE) 9.0 or above (in windows )and Mozilla Firefox 50 (Linux) | Other Required Softwares:- Adobe Reader and Flash player. |
| net Framework 3.5 and above | Full admin Rights required for the User. | No other software should be installed in OS. |
| Internet Connectivity should be isolated from the exam conducting LAB. | Proxy Should be disable. | Proxy Should be disable. |
| Firewall should be enable. | PC should be updated from ransomware patch. |  |

4.**Technical requirements**

|  |  |  |
| --- | --- | --- |
| CPU Hardware ( if available as above mention yes if not then give details of available configuration) | Monitor requirement ( if available as above mention yes if not then give details of available configuration) | CPU Operating System ( if available as above mention yes if not then give details of available configuration) |
| Primary netboot OS.Ileon OS (To be provided by TCS) for candidate machines | Backup linux Ubuntu 14.0.4 LTS | Internet connectivity to server |
| Network Configuration - STAR Topology / Network Cable – ACT 5E/CAT 6 /Connectors – RJ45v/Switches – Min 100 Mbps | | |